{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Bid to Purchase"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Bid to Purchase","index":0,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,"Section 00130 - Bid Schedule"]
[]
[null,null,null,"2020 Concrete Repair Program"]
[]
[null,null,null,null,"Bid","Unit"]
[null,"Item #","Description","Unit","Quantity","Bid Price","TOTAL COST"]
[null,1,"Remove Curb & Gutter (0 to 2' Pan)","LF",5367.5,null,{"$f":"E8*F8","v":0}]
[null,2,"Remove Concrete Flatwork - Thickness Varies ","SY",2740.3861111111109,null,{"$f":"E9*F9","v":0}]
[null,3,"Removal of Rollover C&G/Sidewalk","LF",3070,null,0]
[null,4,"Remove Asphalt (Thickness Varies)","SY",980.66666666666674,null,0]
[null,5,"Sawcut Joint","LF",400,null,0]
[null,6,"Concrete Sawcut Demo","LF",210,null,0]
[null,7,"New C&G 0-2' Pan (i.e. Vertical Curb and Gutter: Sim to S-16)","LF",4554.5,null,0]
[null,8,"New High Back Curb and Gutter (8\" and above)","LF",1000,null,0]
[null,9,"24 Hour High Early Mix - Up Charge","CY",100,null,0]
[null,10,"New Rollover C&G and SW","LF",3070,null,0]
[null,11,"New 4\" Concrete","SY",348.5555555555556,null,0]
[null,12,"New 6\" Concrete ","SY",807.44444444444434,null,0]
[null,13,"New 8\" Concrete","SY",1626.0527777777775,null,0]
[null,14,"New 5\" Concrete w/ Fiber Reinforcement","SY",477.77777777777777,null,0]
[null,15,"Unclassified Excavation","CY",75,null,0]
[null,16,"Compacted Stabilization Subgrade Import (6\" Base)","TON",214.62962962962962,null,0]
[null,17,"Major Re-landscaping (Sprinklers, etc.)","HR",36,null,0]
[null,18,"Reconstruct Inlet Top (up to 2' below grade)","EA",5,null,0]
[null,19,"Adjust Meter Pit","EA",11,null,0]
[null,20,"Landscape Curb 0-6\"","LF",580,null,0]
[null,21,"Landscape Curb 7-18\"","LF",200,null,0]
[null,22,"Landscape Curb 19-48\"","LF",150,null,0]
[null,23,"ADA Detectable Warning plates/domes ","SF",472,null,0]
[null,24,"Chase Drain (12\" max opening)","SF",36,null,0]
[null,25,"Remove and Reset mailbox","EA",5,null,0]
[null,26,"Tree and Root Pruning","HR",9,null,0]
[null,27,"Saw Cut to Preserve Asphalt","LF",255,null,0]
[null,28,"Colored Concrete (4 LB Max.) (Add On)","CY",75,null,0]
[null,29,"Stamped Concrete (Add On)","CY",75,null,0]
[null,30,"Portable Sanitary Station","LS",1,null,0]
[null,31,"4\" PVC Installed Under Sidewalk","LF",100,null,0]
[null,32,"Remove 6\" CMP (19th Ave & 25th St) ","LF",75,null,0]
[]
[null,33,"Arrow Board","Day",54,null,0]
[null,34,"Certified Flagger (When Directed By City)","Hour",80,null,0]
[]
[null,35,"Quality Control - Standard Proctor","EA",14,null,0]
[null,36,"Quality Control - Soils Compaction","EA",15,null,0]
[null,37,"Quality Control - Concrete Test & Break Results","EA",17,null,{"$f":"E46*F46","v":0}]
[null,null,"Total",null,null,null,{"$f":"SUM(G8:G46)","v":0}]
[]
[null,null,"Vendor Name:"]
[]
[null,null,"Authorized Signature:"]
[]
[null,null,"Print Name:"]
[]
[null,null,"Phone Number:                                                      Fax Number:"]
[]
[null,null,"Email Address:                                                                   Date:"]