{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Bid to Purchase","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Bid to Purchase","index":0,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,"Section 00130 - Bid Schedule"]
[]
[null,null,null,"2020 Infrastructure Improvements Program"]
[]
[null,null,null,null,"Bid","Unit"]
[null,"Item #","Description","Unit","Quantity","Bid Price","TOTAL COST"]
[null,1,"Remove Curb & Gutter (0 to 2' Pan)","LF",3523,null,{"$f":"E8*F8","v":0}]
[null,2,"Remove Concrete Flatwork - Thickness Varies ","SY",1697.8367555555551,null,{"$f":"E9*F9","v":0}]
[null,3,"Removal of Rollover C&G/Sidewalk","LF",75,null,0]
[null,4,"Remove Asphalt (Thickness Varies)","SY",26.444444444444443,null,0]
[null,5,"Sawcut Joint","LF",200,null,0]
[null,6,"Concrete Sawcut Demo","LF",148,null,0]
[null,7,"New C&G 0-2' Pan (i.e. Vertical Curb and Gutter: Sim to S-16)","LF",3425,null,0]
[null,8,"New High Back Curb and Gutter (8\" and above)","LF",75,null,0]
[null,9,"24 Hour High Early Mix - Up Charge","CY",41,null,0]
[null,10,"New Rollover C&G and SW","LF",75,null,0]
[null,11,"New 4\" Concrete","SY",1684.2222222222222,null,0]
[null,12,"New 6\" Concrete ","SY",471.16666666666663,null,0]
[null,13,"New 8\" Concrete","SY",191.67008888888893,null,0]
[null,14,"New 5\" Concrete w/ Fiber Reinforcement","SY",0,null,0]
[null,15,"Unclassified Excavation","CY",310,null,0]
[null,16,"Compacted Stabilization Subgrade Import (6\" Base)","TON",260,null,0]
[null,17,"Major Re-landscaping (Sprinklers, etc.)","HR",1000,null,0]
[null,18,"Reconstruct Inlet Top (up to 2' below grade)","EA",2,null,0]
[null,19,"Adjust Meter Pit","EA",5,null,0]
[null,20,"Landscape Curb 0-6\"","LF",527,null,0]
[null,21,"Landscape Curb 7-18\"","LF",69,null,0]
[null,22,"Landscape Curb 19-48\"","LF",36,null,0]
[null,23,"ADA Detectable Warning plates/domes ","SF",148,null,0]
[null,24,"Chase Drain (12\" max opening)","SF",0,null,0]
[null,25,"Remove and Reset mailbox","EA",1,null,0]
[null,26,"Tree and Root Pruning","HR",24,null,0]
[null,27,"Saw Cut to Preserve Asphalt","LF",3523,null,0]
[null,28,"Colored Concrete (4 LB Max.) (Add On)","CY",25,null,0]
[null,29,"Stamped Concrete (Add On)","SY",32,null,0]
[null,30,"Portable Sanitary Station","LS",1,null,0]
[null,31,"4\" PVC Installed Under Sidewalk","LF",250,null,0]
[]
[null,32,"Arrow Board","Day",0,null,0]
[null,33,"Certified Flagger (When Directed By City)","Hour",80,null,0]
[]
[null,34,"Quality Control - Standard Proctor","EA",5,null,0]
[null,35,"Quality Control - Soils Compaction","EA",5,null,0]
[null,36,"Quality Control - Concrete Test & Break Results","EA",8,null,{"$f":"E45*F45","v":0}]
[null,null,"Total",null,null,null,{"$f":"SUM(G8:G45)","v":0}]
[]
[null,null,"Vendor Name:"]
[]
[null,null,"DUNS #"]
[]
[null,null,"Authorized Signature:"]
[]
[null,null,"Print Name:"]
[]
[null,null,"Phone Number:                                                      Fax Number:"]
[]
[null,null,"Email Address:                                                                   Date:"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}